Online help : 3D section

To achieve a block diagram:
- Choose a study area on which showed various data (seismic, volcanic, beacons and GPS velocity vector ...)
- Click on the map and hold down to define a rectangle of study.
- Change the width of any window you want, in km, (set the width and then Enter)
- Then show
>> A 3D view of the corresponding selected area is displayed.

Using the mouse, it is possible to move, view the block diagram in various angles and zoom.
All points (earthquakes, volcanoes, GPS tags ...) find themselves on the block diagram according to their geographical references (latitude, longitude, depth).

On the scale of the lithosphere, the topography of the land surface cannot occur if you do not exaggerate the vertical scale of the block diagram.
- Click on topography to appear as a frame of the topographical points with the same color code.
- The cursor 'topography density' can request a density of points more or less (which requires the software response time accordingly!).
- The cursor 'Vertical exaggeration' to change the scale heights of the block diagram, which can reveal the fine topography of the land surface.